[logic]
active = ph_idle@system_idle

[ph_idle@system_idle]
on_info = {+yan_labx16_switcher_1_off -yan_labx16_switcher_1_end} ph_sound@switcher_1
on_info2 = {+yan_labx16_switcher_2_off -yan_labx16_switcher_2_end} ph_sound@switcher_2
on_info3 = {+yan_labx16_switcher_3_off -yan_labx16_switcher_3_end} ph_sound@switcher_3 , {+yan_labx16_switcher_primary_try} ph_sound@switcher_primary


[ph_sound@switcher_1]
snd = system_message_2
on_timer = 5000 | ph_idle@system_idle %+yan_labx16_switcher_1_end%

[ph_sound@switcher_2]
snd = system_message_3
on_timer = 5000 | ph_idle@system_idle %+yan_labx16_switcher_2_end%

[ph_sound@switcher_3]
snd = system_message_4
on_timer = 5000 | ph_idle@system_idle %+yan_labx16_switcher_3_end%

[ph_sound@switcher_primary]
snd = system_message_1
on_timer = 15000 | ph_idle@system_idle %-yan_labx16_switcher_primary_try%